### DCC Pitch

Allows you to define the default value for the Pitch option that will be used when an Auto Feature is created. The Pitch value allows more accurate measurements of threaded holes and studs. Pitch, inside PC-DMIS, is the distance between threads along the axis of the feature. If the Pitch value is something other than zero, PC-DMIS staggers the feature's hits along the THEO axis, spacing them around the feature using the Start and Ending Angles.

Entry Name: DccPitch

Entry Type: Real Number to specify the distance between threads in MM. Default value is 0.

See the "Pitch Box" topic for additional information.