### Pro Comm Msg Exe

This entry contains the full pathway of the executable to launch the communication tool used to communicate with Pro/ENGINEER.

In version 3.25 and earlier, you had to create an environment variable called Pro_Comm_Msg_Exe that pointed to the actual executable of the communication tool.

In version 3.5 and later if PC-DMIS cannot find this environment variable, it looks for the pathway stored in this entry of the Settings Editor. If the proper pathway exists, PC-DMIS creates the appropriate environment variable, allowing Pro/ENGINEER to run in batch mode.

Entry Name: ProCommMsgExe

Entry Type: Character String of the full path pointing to the application to launch. Default value is None ( ).