### Tolerance For Executing Out Of Order In MM

This value is used to determine if a new feature is being measured out of order. Since some features are in the same general proximity this tolerance value is used to make sure that a new feature is measured only when hits are taken that are more than this tolerance distance from the current feature. If the hit taken is within the tolerance distance, it is considered to be part of the current feature and not a new feature.

When a value of 0 is specified, then this option is not used, so a new feature will not be measured.

Entry Name: ToleranceForExecutingOutOfOrderInMM

Entry Type: Real Number to specify a tolerance distance. Default value is 10.