### Cross Section Step

Indicates the default distance between the planes. The step value is held in the INCREMENT parameter in the Edit Window. This value is displayed in the Pointcloud Operator dialog box for a Cross Section operator.

Entry Name: CrossSectionStep

Entry Type: Real Number specifying Cross Section step. Default value is 10.

See the "CROSS SECTION" topic of the PC-DMIS Laser help file for more information.