### Profile Out Tol Cumulative

This entry allows you to determine how profile dimensions display the OUTTOL value when you use the form and location option. If set to TRUE (1), the profile dimensions with the form and location option displays the OUTTOL value by adding together the out of tolerance positive and the out of tolerance negative values. If FALSE (0), the profile dimension with the form and location option displays the OUTTOL value as the maximum of the two values (the out of tolerance positive and out of tolerance negative values).

Entry Name: ProfileOutTolCumulative

Entry Type: Whole Number specifying TRUE (1) or FALSE (0). Default value is 1.