### DCC Cir Move

Allows you to define the default value for the Circular Moves option that will be used when an Auto Feature is created. When this option is set to TRUE (1), a `MOVE/CIRCULAR` command is inserted before the created feature. PC-DMIS will follow a circular path when taking the next hit based on the radius of the feature.

See "Inserting a Move Circular Command" in the "Inserting Moves" section for information on inserting circular moves into the Edit window.

Entry Name: DccCirMove

Entry Type: Whole Number to specify TRUE (1) or FALSE(0). Default value is 0.