### Max Text Print Resolution

This does the exact same thing as the MaxPrintResolution except it controls the dpi (dots per inch) for labels with a TextReportObject in your printed report, not CAD images.

This entry only functions when DoNotUseAmyuniRTF is set to 0. If it's a non-zero value, PC-DMIS does not attempt to regenerate the labels.

Important: If the dpi is greater than 96 then any labels used, those labels are regenerated at the higher resolution. Regenerating labels causes them to be re-evaluated.

Entry Name: MaxTextPrintResolution

Entry Type: Whole Number specifying the print resolution. Default value is none (1000000), which effectively causes this value to be ignored.