### DCC R Slot Meas Angle

Allows you to define the default value for the Meas Angle option that will be used when an Auto Round Slot is created. Round slots have two rounded ends, each having up to 180 degrees of measurement radius. The Meas Angle value defines how much of the radius to measure. PC-DMIS takes the input value and divides it in two, measuring half on each side of the slot angle vector.

Entry Name: DccRSlotMeasAngle

Entry Type: Whole Number to specify degree angle. Default value is 90.

Example: Suppose you type 90 in this box. When creating the Round Slot, PC-DMIS would then measure 45 degrees to the left, and 45 degrees to the right of the angle vector (or vice versa depending on the angle vector).