### Rotab Angle (1-36)

These values allow you to store up to 36 Rotary Table Angles. These angles are used in the calibration process when a Rotary Table is present (see ProbeToolOnTable).

Note: These values serve as place holders for the last used values, but should be edited from the Calibrate Rotary Table dialog box within PC-DMIS.

Entry Name: RotabAngle(1-36)

Entry Type: Whole Number specifying angle in degrees. Default value is 0.