### External Rotab Status Timeout

Specifies a timeout for response to the request for table position/status. A value of 0.0 disables this timeout. If the timeout occurs, and if the value of ExternalRotabStatusAutoRetries has been exceeded, the user will be prompted as to whether or not to try resending the command for which the response was not received within the allowed time.

Entry Name: ExternalRotabStatusTimeout

Entry Type: Real Number specifying seconds. Default value is 2.