### Rotab Table1 Increment

Provides the minimum angular movement in degrees to be allowed for the given table. This only applies to indexable rotary tables and this should be equal to, or an integer multiple of, the actual minimum hardware incremental movement. If more than one rotary table is present this applies only to the first table.

Entry Name: RotabTable1Increment

Entry Type: Real Number specifying angle in degrees. Default value is 1.