#### Measure a Circle

Red Dots show Possible Hit Locations

Move the probe to the center of one circle. (The top left circle was selected for this example.) Lower the probe into the hole and measure the circle, taking four hits in approximately equal distances around the circle. Press the END key after the last hit. PC-DMIS will display a feature ID and measured circle in the Graphics Display window.