### Highlighting the Current Probe Tip

On probe configurations that contain multiple probe shanks and tips like the one shown below, PC-DMIS provides a way for you to easily know which tip is the active tip at any given time.

Probe Configuration with Multiple Tips

With version 4.3 and higher, PC-DMIS automatically highlights the entire probe shank and tip in the Graphics Display window when the cursor location in the Edit window rests on a command that uses the active tip:

Probe Configuration with Active Tip Highlighted