### Ignore Cad To Part

PC-DMIS only saves the machine to part alignment and does not create the CAD to parts transformation matrix when you save and alignment and this option is set to TRUE (1). All theoretical values will now be independent of one another. This is useful when you want to execute an alignment from features measured without CAD data in DCC mode.

Entry Name: IgnoreCadToPart

Entry Type: Whole Number specifying TRUE (1) or FALSE (0). Default value is 0.