### Tool Changer ACR3 Port 4 Port 5 Delta

This value is used to compensate for the additional distance between center location of port 4 on the first ACR3 toolchanger and center location of port 1(5) on the second ACR3 toolchanger. For example, when two ACR3 toolchangers mounted next to each other on a MRS rack the distance between port 4 and port 5 is more than the normal distance between port 3 and port 4. This specified value is added to the normal port spacing to define the relative location of port 5.

Entry Name: ToolChangerACR3Port4Port5Delta

Entry Type: Real Number specifying distance between port 4 and 5. Default value is -99999 which means no offset occurs.