### Probe Qual Vision Angle Start

Stores the default start angle that is used in the Measure Vision Probe dialog box. The angle is given in degrees in a Cartesian coordinate system as seen when looking down or –Z. An end angle of zero would be aligned to the +X. An end angle of 90 would be aligned to the +Y axis.

Note: This angle different from the angle used for the contact probe and a sphere tool, which relates to the angle from the sphere equator to the pole.

Entry Name: ProbeQualVisionAngleStart

Entry Type: Real Number specifying angle in degrees. The default is 0.