### Machine Mirror Axis

Defines how PC-DMIS positions the mirrored part on a virtual machine displayed in the Graphics Display window.

Entry Name: MachineMirrorAxis

Entry Type: Values of 1, 2 and 3 are the only valid values for this registry key. The default value is 2 which will mirror the virtual machine in the Y axis. Setting this value to 1 would mirror the virtual machine in the X axis. Setting this value to 3 would mirror the virtual machine in the Z axis. Any other value will reset this key back to the default value of 2.