### 5 Unique Gripper Offset (XYZ)

This value is not used.

These three values store the values of the gripper offsets after calibration or your 5 Unique fixturing system. The gripper offset is treated the same as a probe offset. The center of the gripper is hereby linked to the machine.

Entry Name: 5UniqueGripperOffset(XYZ)

Entry Type: Real Number to specify gripper offset. Default value is 0 for X & Y and 149 for Z.