### Command Identification - ID Length

The Length value determines the length of the identification for the various commands. A length between 0-15 digits may be used. If this length is set, PC-DMIS will append zeros to the ID letters to make up the necessary length.

For example: ID Length = 10, ID Letters = CIRCLE.
PC-DMIS will generate an ID = CIRCLE0001, etc. This is done only if the Length is set.

Entry Name: (A,C,COPOper,CS,D,FCF,F,L,Q,V)Length(0-17)

Entry Type: Whole Number to specify number of digits. Default value is 0.

Note: Preferably this value should be set from the ID Setup tab of the SetUp Options (F5) dialog box within PC-DMIS.

Command Key:

ALength0 | Alignments
CLength0 | Comments
COPOperLength0 | Pointcloud Operator
CSLength0 | Call Subs
DLength(0-16) | Dimension/Angle - Symmetry
FCFLength(0-16) | Feature Control Frame
FLength(0-17) | Feature/Blobs - Surfaces
LLength0 | Label
QLength0 | SPC Queries
VLength0 | Variables

See Also:

Command Identification - ID Letters

Command Identification - ID Starting Number