### DMIS Export Fedrat Pcnt Of Max Machine Speed

DMIS commands don't automatically specify whether exported FEDRAT/ commands (commands that control the machine's speed) refer to maximum machine speed or maximum touch speed. This option allows you to specify how this command is exported.

Entry Name: DMISExportFedratPcntOfMaxMachineSpeed

Entry Type: Whole Number to specify whether to use percentage of maximum machine speed (1) or percentage of maximum touch speed (0). Default value is 0.