### RT Offset

This makes it possible to align the rotary table's 0 axis with a machine axis. When you want to align the 0 of a rotary table to a specific machine axis, this entry is a constant offset value that is subtracted from the controller's rotary table position and applied in the opposite direction.

Entry Name: RtOffset

Entry Type: Real number for the offset distance. The default value is 0.