### Clamp Value

The Clamping Value only works with the Leitz controller and the Leitz brand TTP. This value tells the controller how firmly to hold the probe on a Leitz CMM. For a large tip weight, you may need to increase the clamping value. For a small tip weight, you may need to decrease the clamping value.

Entry Name: ClampValue

Entry Type: Real Number specifying clamp pressure. Default value is 0.