#### EW Report Mode Show Tol Bi Upper Percent

This value is set for the upper percentage of a bilateral dimension.

Entry Name: `EWReportModeShowTolBiUpperPercent`

Entry Type: Whole Number that specifies the percentage used for the upper tolerance. Default value is 100.

Example of Bilateral Upper Percentage:

Nominal:3.0000

Measured:3.0075

Deviation:0.0075

Plus Tol:0.0100

Minus Tol:0.0100

The percentage is calculated using the Lever Rule:

(3.0075-2.9900) / (3.0100-2.9900) * 100. = 87.5%

This dimension will be displayed in the inspection report if the Bilateral Upper Percentage is greater than 87.5%.