### Cross Section Length

Indicates the default value for the maximum distance between the first and last plane. This value is displayed in the Pointcloud Operator dialog box for a Cross Section operator.

Entry Name: CrossSectionLength

Entry Type: Real Number specifying Cross Section length. Default value is 100.

See the "CROSS SECTION" topic of the PC-DMIS Laser help file for more information.