### Stable Probing Enabled

When this option is set to True, PC-DMIS will automatically trigger a hit if the following two conditions are met:

- The reflector is left in a position for an amount of time that exceeds the value specified in StableProbingTimeDelay.

- The reflector distance exceeds the value specified in StableProbingDistance.

This allows you to take hits, without using a remote control or interacting directly with the computer.

Entry Name: StableProbingEnabled

Entry Type: True/False value. Default value is FALSE.