### Layer Numbers To Import

This entry lets you specify which PC-DMIS Unigraphics layers, by number, to import the CAD data. You can type an expression that specifies Unigraphics layers to import the CAD data from.

Entry Name: LayerNumbersToImport

Entry Type: Character String specifying the set of layers to be imported. Default value is 1-256.

The layers are specified by individual layers, separated by commas, by ranges of layers separated by commas, or by ranges specified with a hyphen before or after a layer number. The following table of examples illustrates the possible format.

Examples of Set Expression Import Interpretation

1-10, 20-30 | Unigraphics CAD data on layers 1-10 and 20-30 are imported.
1-8 | Unigraphics CAD data on layers 1-8 are imported.
100-256 | Unigraphics CAD data on layers 100-256 are imported.
7 | Unigraphics CAD data on layer 7 is imported.
* | Unigraphics CAD data on all layers, 1-256, are imported.