### Cross Section Delta

Indicates the default value for the maximum distance from the plane for a point to be considered part of the cross section. This value is displayed in the Pointcloud Operator dialog box for a Cross Section operator.

Entry Name: CrossSectionDelta

Entry Type: Real Number specifying the Cross Section delta value. Default value is 0.05.

See the "CROSS SECTION" topic of the PC-DMIS Laser help file for more information.