### Part Mirror Axis

Defines the axis to mirror the Part Program.

Entry Name: PartMirrorAxis

Entry Type: Values of 1, 2 and 3 are the only valid values for this registry key. The default value is 2 which will mirror the part in the Y axis. Setting this value to 1 would mirror the part in the X axis. Setting this value to 3 would mirror the part in the Z axis. Any other value will reset this key back to the default value of 2.