### Scan Dialog Clr Pln

When this option is set to TRUE (1), PC-DMIS inserts a CLEARP MOVE a predetermined distance relative to the current coordinate system and part origin before taking the first hit. Using clearance planes reduces programming time because the need to define intermediate moves is reduced.

Entry Name: ScanDialogClrPln

Entry Type: Whole Number specifying TRUE (1) or FALSE (0). Default value is 0.