### COP Command Mode Text

The COP command inside the Edit window’s Command Mode looks like this:

COP1 =COP/DATA,SIZE=0
REF,,

The COP command must precede any scan referring to it in the part program.

For example the example of REF,SCN2 shown below points to the SCN2 scan and will use its data:

COP2 =COP/DATA,SIZE=0
REF,SCN2,,

You can have more than one scan refer to a COP command.

Important: Be aware that if you cut a COP command and paste it again, the resultant command will get pasted without the data points. If you need to move your COP command to a different location in the Edit window, you will need to re-create the COP command at the desired location and delete the earlier one.