### Special Leica Controls

Tracker Head Movements: You can control the direction that the laser is pointing by using the Alt + left arrow, right arrow, up arrow, down arrow keyboard keys. Use Alt + Space to stop movement of the laser. The tracker motors must be engaged for these controls to work (Tracker | Release Motors - Alt-F12).

| Point To: Use the pop-up menu that appears when you right-click on a feature in the Edit Window to Point To the feature's nominal position (Laser Pointer). Move To: Use the pop-up menu that appears when you right-click on a feature in the Edit Window to Move To the features nominal position (Go Position). ???? What does this entail?