### Vision

- PCD-23630 - Added two new machine types into PC-DMIS: Optiv Classic 322 and Optiv Classic 432

- PCD-23705 - Added support for using a digital camera on the FDC system

- PCD-23656 - Added the ability to measure the smallest concentric circle on a new artifact in order to calibrate high-magnification systems

- PCD-23589 - Added the ability to change a circle target back into an arc so that users can measure arcs without splitting the target

- PCD-23729 - Added ability for CWS on FDC to take a single point measurement

- PCD-23731 - Added the CWS probe type

- PCD-23697 - Added a SET_VAR TRIGFREQDIV command to set the FDC trigger frequency from the part program

- PCD-23706 - Added a Focus Laser Sensor (FLS) probe type for FDC

- PCD-23703 - Added the ability to set the FLS beam on or off with FDC

- PCD-23704 - Provided the Live view for the FLS probe type for FDC

- PCD-23726 - Added the scan measurement with FLS for FDC

- PCD-23694 - Added the single point measurement with FLS for FDC

- PCD-23700 - Added the ability to support lamp intensity for CWS

- PCD-23689 - Modified the 2D profile feature to disable the Matching Edge and Underscan feature options

- PCD-23638 - Modified the 2D profile feature so that it now defaults to opening the Auto Feature dialog box in advanced mode