laser

#### Cone Specific Parameters

Diameter: The value in this box defines the cone's diameter.

Length: The value in this box provides the length (height) of the cone's axis. The length parameter is only valid as nominal. No actual length measurement will be performed.

Inner/Outer: This parameter defines whether or not the cone is an inner cone (hole) or an outer cone (stud).

The Overscan value on the Laser Scan Properties tab of the Probe Toolbox should use negative values unlike other Laser Auto Features. This limits measurement in the conical region along the cone axis.

Depth - This parameter controls the location of the laser focal point in relation to the cone's outside diameter (outer cones) or the cone's center axis (inner cones). This allows you to control how the laser stripes fall on the cone's surface by specifying how far or close the laser is to the cone's surface. A depth of 0 (zero) causes this feature to be calculated at the surface plane height using data found at the lowest possible depth from the surface plane. A depth of any other value causes it to be calculated at that depth.

Center Offset - This value identifies the center of the cone portion of the stud.

Search Length - This value identifies the length of the cone portion.

The depth defaults to 0 (zero). This is the default value for a plane feature with no extruded edges. You should only change this to a different value if there are specific requirements from your part's drawing. Otherwise, PC-DMIS unsuccessfully attempts to locate points at the specified depth, resulting in a feature calculation error from the feature extraction module.

Sample external Cone in the Graphic Display window showing:

- The Diameter (top black circle)

- The Length (bottom black circle)

- The Depth (blue circle)

- The Center Point (yellow circle)

Sample external Stud Cone in the Graphic Display window showing:

- The Search Length (purple circles)

- The Center Offset (lime green circle)

- The Point Segregation (orange circles)

- The Center Point (yellow circle)

- The Clipping Plane (light green circle)

- The Overscan (sea green circles)

- The Ring Band (pink circles)

More:

Laser Cone

Cone Command Mode Text

Auto Cone Paths