miim

### Examples of Configurations

The ENC7360 card is not supported in x64.

Manual CMM in 7480 Card Support Configurations

(A) - PC-DMIS (pcdlrn.exe)

(B) - ManualCMM.dll renamed as Interfac.dll. It must match PC-DMIS

(C) - TCP/IP

(D) - GmServer.exe

(E) - TCP port 1360

(F) - Enc7480.DLL

(G) - 7480 Card (Hardware)

(H) - GMICConfigData.xml

(I) - GMS.xml

(J) - GMSENC7480.xml

Manual CMM in Simulation

(A) - PC-DMIS (pcdlrn.exe)

(B) - ManualCMM.dll renamed as Interfac.dll. It must match PC-DMIS

(C) - TCP/IP

(D) - GmServer.exe, independent of PC-DMIS

(E) - TCP Port 1360

(F) - GmsSimulator.dll. It must match GmServer.exe

(G) - GMIConfigData.xml

(H) - GMS.xml

(I) - GmsSimulator.xml