core

### Operator

(This item applies to the Comment dialog box, accessible through Insert | Report Command | Comment.)

The Operator option displays the comment text to the operator when the software executes the comment command.

To use Operator option:

1. Place the cursor in the Edit window where you want to insert the comment command.

2. Select the Insert | Report Command | Comment menu option to open the Comment dialog box.

3. From the Comment dialog box, select the Operator option.

4. In the Comment Text box, type the comment text.

5. Click the OK button to close the dialog box and insert the comment.

The Edit window command line for this option reads:
COMMENT/OPER,TOG1,FULL SCREEN=TOG2,AUTO-CONTINUE=TOG3,
comment text

TOG1 - This YES/NO field allows you to specify whether or the comment shows up in the inspection report.

TOG2 - This YES/NO field determines whether or not the comment will be displayed to fill the entire screen.

TOG3 - This YES/NO field determines whether or not the comment will use a count down timer and automatically continue execution once the timer reaches zero. When the count down timer reaches zero, PC-DMIS will continue as if you had clicked the OK button.

How it Works

When PC-DMIS executes the measurement routine, a message box will display the appropriate comments just under the Execution dialog box.

A Sample PC-DMIS Message dialog box

PC-DMIS will not allow you to edit this message. Click on the OK button to continue execution. Click Cancel to cancel measurement routine execution.