Collapse All Expand All

PC-DMIS 2019 R1 Object Library |
DefaultDimensionColors Object Members
See Also Overview Send Topic Feedback | See Object Hierarchy Chart

PCDLRN ActiveX DLL : DefaultDimensionColors Object

Glossary Item Box

# Public Methods

Refresh | This method forces the measurement routine to refresh. This causes it to use any newly defined dimension colors.

# Public Properties

DefaultToleranceValue | This read/write property determines the default tolerance value. This is the same thing as the Default tolerance value in the Edit Dimension Color dialog box. For more information, see the PC-DMIS help file.
DimensionLimitColor | This read/write property determines the Dimension limits color. This is the same thing as the Dimension Limits color in the Edit Dimension Color dialog box. For more information, see the PC-DMIS help file.
MaxNumberOfToleranceZones | This read-only property shows the maximum number of allowed tolerance zones.
MinNumberOfToleranceZones | This read-only property shows the minimum number of allowed tolerance zones.
NegativeOutOfToleranceColor | This read/write property determines the negative out-of-tolerance color (yellow by default). This property does the same thing as setting the negative out-of-tolerance color in the Edit Dimension Color dialog box. For more information, see the PC-DMIS help file.
NumberOfToleranceZones | This read/write property determines the number of tolerance zones for the measurement routine. This property does the same thing as the Number of tolerance zones value in the Edit Dimension Color dialog box. For more information, see the PC-DMIS help file.
PositiveOutOfToleranceColor | This read/write property determines the positive out-of-tolerance color (red by default). This property does the same thing as setting the positive out-of-tolerance color in the Edit Dimension Color dialog box. For more information, see the PC-DMIS help file.
ShowColorsInTwoDirections | This read/write property determines whether or not tolerance zones for the measurement routine show the same color range in two directions. This property does the same thing as the Show Colors in Two Directions check box in the Edit Dimension Color dialog box. For more information, see the PC-DMIS help file.
ToleranceZoneColors | This read/write parametric property determiens the color of a specific tolerance zone. This property does the same thing as setting a color for a specific tolerance zone in the Edit Dimension Color dialog box. For more information, see the PC-DMIS help file.
ToleranceZoneMultiplier | This read/write property represents a percentage value. It increases or decreases the tolerance zone by the defined percentage. This property does the same thing as the Tolerance Zone Multiplier box in the Edit Dimension Color dialog box. For more information, see the PC-DMIS help file.

# See Also

DefaultDimensionColors Object

Copyright © 2019. Hexagon Manufacturing Intelligence – Metrology Software, Inc. All Rights Reserved.