settingseditor

### CrossSectionCopCadCrossSectionStep

This registry entry is used only when the CrossSectionCopCadCrossSectionDrivenByCad entry is set to 1 (True). The value for the CrossSectionCopCadCrossSectionStep entry is the step that is used along the CAD polylines to look for the best interpolated COP point. For greater accuracy, or if the CAD model is very small, you can set this value to a smaller value.

If this value is changed and a corresponding Profile dimension was previously created, you must re-execute the Profile. If you do not re-execute the Profile, the change will not appear in the Graphic Display window.

Entry Name: CrossSectionCopCadCrossSectionStep

Entry Type: Real Number that specifies the step number. The default value is 1.