laser

#### Measurement Properties Area

For information about the specific parameters that are configured in this section, see the following topics:

- Edge Point Specific Parameters

- Plane Specific Parameters

- Circle Specific Parameters

- Slot Specific Parameters

- Flush and Gap Specific Parameters

- Cylinder Specific Parameters

- Sphere Specific Parameters

Auto Wrist - This toggle button will cause the probe orientation to move to a vector that closely corresponds to the surface vector of the Auto Feature.

View Normal - Clicking this button orients that CAD so that you look down on the feature.

View Perpendicular - Clicking this button orients the CAD so that you look at the side of the feature.