core

### Execute From Start Points

To begin execution at a specified start point, first set the start point by right-clicking inside Command mode and selecting Set Start Point from the shortcut menu, and then choose the Execute from Start Points menu command.

Be aware when the current tip for that location in the measurement routine does not match the current orientation of the probe head. The software does not execute the previous tip command in order to change the tip orientation.