core

### Johansson Interface

The Johansson interface is used with Johansson machines. This interface requires Proto software that is installed as part of the JoWin installation. When PC-DMIS starts, it also starts the Proto software and terminates Proto when you exit PC-DMIS. Proto detects the communication setting to communicate with the controller.

Before you start PC-DMIS, rename johansson.dll to interfac.dll.

The Machine Options dialog box (Edit | Preferences | Machine Interface Setup) has these tabs for the Johansson interface:

Axis tab

See the "Assigning the Machine Axes" topic.

Debug tab

See the "Generating a Debug File" topic.

Additional information for this interface is provided in the Machine Interface Installation Manual (MIIM).

You can access the MIIM help file from this link: .