settingseditor

### DccThickness2Distance

Specifies the edge thickness of a plastic or sheet metal part where the CAD data only describes one side. Only Edge Point auto features use this value. PC-DMIS applies this material thickness automatically when using the CAD surface data. This thickness will be applied automatically along the surface normal vector each time CAD data is selected. Positive or negative values can be used.

Entry Name: DccThickness2Distance

Entry Type: Real Number to specify thickness. The default value is 0.