settingseditor

### Command Identification - IDLetters

This registry entry determines the first letter or letters to use in the identification process. PC-DMIS always displays the ID in capital letters. You can enter up to 15 characters.

Entry Name: A,C,COPOper,CS,D,FCF,F,L,Q,V)Ltrs(0-17)

Entry Type: Character string that specifies the starting letters. The default value varies.

Preferably, this value should be set on the ID Setup tab in the Setup Options (F5) dialog box in PC-DMIS.

Command Key

Command | Type
ALtrs0 | Alignments
CLtrs0 | Comments
CSLtrs0 | Call Subs
DLtrs(0-16) | Dimension/Angle - Symmetry
FCFLtrs(0-16) | Feature Control Frame
FLtrs(0-17) | Feature/Blobs - Surfaces
LLtrs0 | Label
QLtrs0 | SPC Queries
VLtrs0 | Variables

See Also:

Command Identification - ID Length

Command Identification - ID Starting Number