core

### Importing a MeasureMax Project

PC-DMIS can import a MeasureMax project, converting it to work in a PC-DMIS measurement routine.

To import a MeasureMax project,

1. Open the measurement routine in PC-DMIS into which you are going to import the MeasureMax project.

2. Select the File | Import | MeasureMax Project menu option. An Open dialog box appears.

3. Navigate through the available directories until you find the directory containing the desired MeasureMax file.

4. Select the .vbp file from the directory.

5. Click Import. PC-DMIS automatically converts the project and inserts the PC-DMIS commands at the end of your measurement routine.

6. Follow any on-screen prompts to import the MeasureMax project into PC-DMIS.