miim

#### Connection

Connect the 2 cameras to the frame grabber video inputs 0-3 as identified in the Matrox hardware documentation for the frame grabber board being used or on the labeling of the Matrox DB connector to BNC cables (Cronos:DB25-TO-5BNC or Meteor: DH44-TO-13BNC). Be careful not to connect a single composite BNC connection to a marked Chroma line on the Matrox cable. On the IDS Falcon or Eagle frame grabbers, you can connect to any video input.