core

#### Sensor numbers boxes

The Sensor numbers boxes contain a list of one or more sensor numbers to be used for the given axis or part. These values are very important when reading temperatures from the controller because they must correspond to how the sensors are actually configured.

- Each sensor is a number in the range of 1 to 32.

- Items in the list can be either a single number or a range from first to last.

- Items are separated by commas or left blank.

- The input allows up to 32 values for any axis or the part.

For "manual" mode, these numbers are relatively meaningless, but at least one sensor number must be assigned for each axis and the part.