settingseditor

### CrossSectionStep

This registry entry indicates the default distance between the planes. The step value is held in the INCREMENT parameter in the Edit window. This value appears in the Pointcloud Operator dialog box for a CROSS SECTION operator.

Entry Name: CrossSectionStep

Entry Type: Real Number that specifies the cross section step in mm. The default value is 10.

See "CROSS SECTION" in the PC-DMIS Laser documentation for more information.