Collapse All Expand All

PC-DMIS 2019 R1 Object Library |
CopyMeasToNom Property
See Also Send Topic Feedback | See Object Hierarchy Chart

PCDLRN ActiveX DLL > Command Object : CopyMeasToNom Property

Glossary Item Box

# Description

Property used to indicate/set whether the object should execute in MASTER mode. After executing in MASTER mode, the object copies the measured vector, centroid, and other nominal information to the nominals and turns off MASTER mode. This copies the same information that gets calculated using the CalculateNominals method.

# Syntax

Visual Basic
    Public Property CopyMeasToNom As Boolean

# Return Type

Read/write Boolean.

# Remarks

The nominal information that this copies includes the following:

- CENTROID
- VECTOR
- DIAMETER
- STARTPOINT
- ENDPOINT
- BALLCENTER
- LENGTH
- ELLIPSEMINORAXIS
- ANGLE
- SURFACEVECTOR
- THICKNESS
- NUMHITS
- SPACER
- INDENT
- AUTO_MOVE_DISTANCE
- DEPTH
- TARG
- SCANROWCOUNT
- ANGLE_VECTOR
- PUNCH_VECTOR
- PIN_VECTOR
- PIN_DIAMETER
- REPORT_VECTOR
- REPORT_SURF_VECTOR
- HEIGHT
- MEASURE_VECTOR
- UPDATE_VECTOR
- CORNER_RADIUS
- ANGLE2

# See Also

Command Object | Command Members

Copyright © 2019. Hexagon Manufacturing Intelligence – Metrology Software, Inc. All Rights Reserved.