Collapse All Expand All

PC-DMIS 2019 R1 Object Library |
RotateToPoint Method
See Also Send Topic Feedback | See Object Hierarchy Chart

X
  Required Double X component used in calculating rotation angle.

Y
  Required Double Y component used in calculation rotation angle.

Workplane
  Optional parameter with the ENUM_PLANE_TYPE enumeration used to define which axis to rotate about.

PCDLRN ActiveX DLL > DmisMatrix Object : RotateToPoint Method

Glossary Item Box

# Description

Rotates the matrix by the calculated angle relative to the workplane.

# Syntax

Visual Basic
    Public Sub RotateToPoint( _
       ByVal X As Double, _
       ByVal Y As Double, _
       ByVal Workplane As ENUM_PLANE_TYPE _
    )

# Parameters

X
  Required Double X component used in calculating rotation angle.
Y
  Required Double Y component used in calculation rotation angle.
Workplane

  Value | Description
  --- | ---
  PLANE_BACK |
  PLANE_BOTTOM |
  PLANE_FRONT |
  PLANE_LEFT |
  PLANE_RIGHT |
  PLANE_TOP |

  Optional parameter with the ENUM_PLANE_TYPE enumeration used to define which axis to rotate about.

# See Also

DmisMatrix Object | DmisMatrix Members

Copyright © 2019. Hexagon Manufacturing Intelligence – Metrology Software, Inc. All Rights Reserved.