laser

#### Mesh EMPTY Operator

Mesh Operator dialog box - EMPTY operator

When this command is executed, PC-DMIS removes all the data from the Mesh.

To apply the Mesh EMPTY operation to a Mesh:

1. In the Edit window, position your cursor just above the Mesh you want to empty.

2. Click Empty a Mesh () on the Mesh toolbar, or select the menu option Operation | Mesh | Empty. The Mesh Operator dialog box appears.

3. Click Create to insert a MESH/OPER,EMPTY command into the Edit window. The software inserts it just above the Mesh you want to empty. This is the Mesh that the Empty command acts on.

For example:

MESHEMPTY1 =MESH/OPER,EMPTY,

REF,MESH1,,

Once this command has been applied to a Mesh, there is no way to restore Mesh data that was removed. Undo does not restore this data.