core

#### Calibrate Infinite Rotary Table

Calibrate Infinite Rotary Table dialog box

(For information on accessing this dialog box, see "Calibrate Rotary Table" )

For information on many of the options on this dialog box, see the "Calibrate Indexable Rotary Table" topic.

The Calibrate Infinite Rotary Table dialog box differs from the Calibrate Indexable Rotary Table dialog box in these areas:

- Instead of the Angles to Calibrate list, the dialog displays the Table Angles list.

- You don’t have to use the 0.0 angle in the Table Angles list.

- Instead of three calibration tools, the dialog box only displays one calibration tool.

Once the options within the dialog box are satisfactory, click the Calibrate button to start the rotary table calibration process.

WARNING: When you do this, the machine moves. To avoid injury, stay clear of the machine. To avoid hardware damage, run the machine at a slower speed.